# Changelog

All notable changes to Polo and Polo Send are documented here.

## 1.0.0
- Initial scaffold: Polo Send taps each track into a shared bridge (distance,
  azimuth, and manual Tilt L/R); Polo (Sum) reads every live Send and derives
  per-source pre-delay, wet gain, and air-absorption from its distance into
  one shared plate/hall/room/reflections reverb (Dattorro tank).
- Tilt L/R modulates the OPPOSITE side's pre-delay up toward Max Pre-Delay
  (the tilted-toward side stays at its distance-based value), for a phantom
  center shift without hard-zeroing either side.
- Native faceplate UI for both plugins: Polo Send's distance/tilt Pad, Polo's
  room-depth tunnel Display, Type/Character selectors, Bypass, and license
  entry.
- VST3, CLAP, AU (macOS), AAX.
